SAFE STOP & USE OF LIGHTS POLICY

Pick up and drop off procedure overview

At a distance of at least 150 meters from a scheduled stop, the driver will activate amber flashing lights, followed by the RED INTERMITTENT FRONT AND BACK FLASHING LIGHTS, THE RED STOP SIGN ARM, and THE CROSSING ARM in front of the bus. These steps are completed and in effect prior to any students boarding or leaving the bus. These signals mean kids are exiting or entering the bus for duration of the loading and unloading process. **WHEN THE RED FLASHING LIGHTS ARE ACTIVATED, IT IS ILLEGAL TO PASS THE BUS FROM ANY DIRECTION.**